{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["sheet"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1904"}

{"sheet":"sheet","index":0,"n_rows":11,"n_cols":30,"rows_kept":11,"cut":false,"hidden":false,"merged":[[6,5,6,8],[2,0,5,2]]}
[null,null,null,null,"Lat-d° ","Lat-m' ","Long-d°","Long-m' ",null,null,null,null,null,null,null,null,null,"To start calculations,"]
[null,null,null,null,33,47,131,59,null,null,null,null,null,null,null,null,null,"option+command+t (Mac)"]
["DO NOT insert/delete any columns and rows in this blue area",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"ctrl+t (win)"]
[null,null,null,null,"Reference height of measurement [m]"]
[null,null,null,null,1.1000000000000001]
[null,null,null,null,"Height of anemometer [m]"]
[null,null,null,"Enter RH or WBT or hPa or x",1.1000000000000001,"Input data by four component radiometer"]
["date","time","ta","RH","vel","Kd","Ku","Ld","Lu","Solar absorptance of cloths","Solar transmittance of cloths","clo","met","Representative temperature","Mean skin temperature","Wettedness",null,null,null,null,null,"ETU","NUATF","TVF","SERFL","ERFS","SEHF","TVFr","TVFe","EVCF"]
["[ymd]","[h:m:s]","[°C]",null,"[m/s]","[W/m2]","[W/m2]","[W/m2]","[W/m2]","[dimensionless]","[dimensionless]","[clo]","[met]","[°C]","[°C]","[dimensionless]",null,null,null,null,null,"[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]","[°C]"]
["2012-07-31","13:00:00",30,60,3,900,133,300,450,0.5,0.1,0.4,2,28.81,31.5,0.15,"/___","input data",null,"results","___\\",35.105298234110542,1.1900005340576172,-1.1522585104154182,-8.5764966042589776,11.034217420101404,-0.286529434420981,5.9248359286785863,-1.8394705655740642,2.9331068992614746]
["2012-07-31","15:00:00",31,60,2,800,120,300,450,0.5,0.1,0.4,2,28.81,31.5,0.15,null,null,null,null,null,37.4112246973094,2.1900005340576172,-0.30167041847057519,-9.1764966042589773,12.517468189300272,-0.52107094067292581,5.3239235307341328,-1.4319290593225227,3.5903241634368896]